*CLS
*IDN?
*RST
AWGControl:CONFigure:CNUMber?
AWGControl:RMODe CONTinuous
DISPlay:UNIT:VOLT AMPLitudeoff
AWGControl:INCreasing INTERpolation
AWGControl:DECreasing DECIMation
WLISt:WAVeform:IMPort "Sine_10000", "\Example_Wave_TXT\10000_Sample_Analog_Sine_Wave.txt",ANAlog 
SEQuence:LENGth 1
SEQuence:ELEM1:WAVeform1 "Sine_10000"
SEQuence:ELEM1:AMPlitude1 2.000000
SEQuence:ELEM1:OFFset1 0.000000
SEQuence:ELEM1:WAVeform2 "Sine_10000"
SEQuence:ELEM1:AMPlitude2 2.000000
SEQuence:ELEM1:OFFset2 0.000000
SEQuence:ELEM1:LENGth 10000
SEQuence:ELEM1:LOOP:COUNt 1
OUTPut1:STATe ON
OUTPut2:STATe ON
AWGControl:RUN
