*RST
SOURce1:FUNCtion:SHAPe GAUSsian
SOURce1:FREQuency 10MHZ
SOURce1:VOLTage:AMPLitude 1
SOURce1:VOLTage:OFFSet 0
SOURce2:FUNCtion:SHAPe SQUare
SOURce2:FREQuency 5MHZ
SOURce2:VOLTage:HIGH 2
SOURce2:VOLTage:LOW 0
OUTPut1:STATe ON
OUTPut2:STATe ON
AFGControl:START