*RST
SOURce1:FUNCtion:SHAPe PULSe
SOURce1:VOLTage:HIGH 2
SOURce1:VOLTage:LOW 0
SOURce1:FREQuency 50KHZ
SOURce1:PULSe:TRANsition:LEADing 1.5us
SOURce1:PULSe:TRANsition:TRAiling 1.5us
SOURce1:PULSe:DCYCle 50
SOURce1:PWM:STATe ON
SOURce1:PWM:INTernal:FUNCtion TRIangle
SOURce1:PWM:INTernal:FREQuency 1KHZ
SOURce1:PWM:DEViation:DCYCle 30
OUTPut1:STATe ON
AFGControl:START