Talker Listener Script: <<Script1>>
*RST
AWGControl:CONFigure:CNUMber?
AWGControl:CONFigure:SEQuencer:MODE SIN
AWGControl:CHANnel:FUNCTionality ARB,LOWSPeed;
AWGControl:RMODe SEQ;
WLIST:WAVeform:DELETE ALL
MMEMory:IMPort "triangle","C:\Program Files (x86)\Active Technologies\EXPERT RIDER AWG 4000\SCPI\AWG4KImportWaveforms\Triangle.txt",TXT
MMEMory:IMPort "sinc","C:\Program Files (x86)\Active Technologies\EXPERT RIDER AWG 4000\SCPI\AWG4KImportWaveforms\Sinc.txt",TXT
SEQuence:CHANnel1:LENGth 1;:SEQuence:CHANnel2:LENGth 1
SEQuence:CHANnel1:ELEMent1:WAVeform "triangle";:SEQuence:CHANnel2:ELEMent1:WAVeform "sinc"
SEQuence:CHANnel1:ELEM1:REP INFinite;:SEQuence:CHANnel2:ELEM1:REP INFinite
AWGControl:RUN
