Talker Listener Script: <<Script1>>
AWGControl:CONFigure:CNUMber?
AWGControl:CONFigure:SEQuencer:MODE SIN
AWGControl:CHANnel:FUNCTionality ARB,LOWSPeed;
WLIST:WAVeform:DELETE ALL
MMEMory:IMPort "wave1","C:\Program Files (x86)\Active Technologies\EXPERT RIDER AWG 4000\SCPI\AWG4KImportWaveforms\Triangle.txt",TXT
MMEMory:IMPort "wave2","C:\Program Files (x86)\Active Technologies\EXPERT RIDER AWG 4000\SCPI\AWG4KImportWaveforms\Sinc.txt",TXT
AWGC:RMODe TRIGgered 
SOURce1:WAVeform "wave1"
SOURce2:WAVeform "wave2"
AWGControl:RUN
