Talker Listener Script: <<Script1>>
*RST
AWGControl:CONFigure:CNUMber?
AWGControl:CONFigure:SEQuencer:MODE SIN;
AWGControl:CHANnel:FUNCTionality ARB,LOWSPeed;
AWGControl:RMODe SEQ;
WLIST:WAVeform:DELETE ALL
SEQuence:CHANnel1:LENGth 1;:SEQuence:CHANnel2:LENGth 1
SEQuence:CHANnel1:ELEMent1:WAVeform "Triangle_2048_P";:SEQuence:CHANnel2:ELEMent1:WAVeform "Sine_2048_P"
SEQuence:CHANnel1:ELEM1:REP INFinite;:SEQuence:CHANnel2:ELEM1:REP INFinite
AWGControl:RUN
