Talker Listener Script: <<Script1>>
*RST
AWGControl:CONFigure:CNUMber?
AWGControl:CONFigure:SEQuencer:MODE SIN;
AWGControl:CHANnel:FUNCTionality ARB,LOWSPeed;
AWGControl:RMODe SEQ;
WLIST:WAVEform:DELETE ALL
MMEMory:IMPort "counter","C:\Program Files (x86)\Active Technologies\EXPERT RIDER AWG 4000\SCPI\AWG4KImportWaveforms\Counter16Bits.txt",DIG
SEQuence:CHANnel1:LENgth 1;:SEQuence:CHANnel2:LENgth 1
SEQuence:CHANnel1:ELEMent1:WAVeform "counter";:SEQuence:CHANnel2:ELEMent1:WAVeform "counter"
SEQuence:CHANnel1:ELEM1:REP INFinite;:SEQuence:CHANnel2:ELEM1:REP INFinite
CLOCK:SRATe 100E6
AWGControl:RUN
