*RST
AWGControl:CONFigure:CNUMber?
AWGControl:CONFigure:SEQuencer:MODE SIN
AWGControl:CHANnel1:FUNCTionality ARB,LOWSPeed;:AWGControl:CHANnel2:FUNCTionality ARB,LOWSPeed
AWGControl:RMODE SEQ;
WLIST:WAVeform:DELETE ALL
WLIST:WAVeform:NEW 'wave1',128
WLIS:WAV:DATA "wave1",0,128,"AN_DIG128MXD.bin"
SEQuence:CHANnel1:LENGth 2;:SEQuence:CHANnel2:LENGth 2
SEQuence:CHANnel1:ELEMent1:WAVeform "wave1";:SEQuence:CHANnel2:ELEMent1:WAVeform "wave1"
SEQuence:CHANnel1:ELEM1:REP 4;:SEQuence:CHANnel2:ELEM1:REP 4
SEQuence:CHANnel1:ELEMent2:WAVeform "wave1";:SEQuence:CHANnel2:ELEMent2:WAVeform "wave1"
SEQuence:CHANnel1:ELEM2:REP INFinite;:SEQuence:CHANnel2:ELEM2:REP INFinite
AWGControl:RUN
