Talker Listener Script: <<Script1>>
*RST
AWGControl:CONFigure:CNUMber?
AWGControl:CONFigure:SEQuencer:MODE SIN;
AWGControl:CHANnel:FUNCTionality ARB,LOWSPeed;
AWGControl:RMODe SEQ;
WLIST:WAVeform:DELETE ALL
MMEMory:IMPort "Sine0","C:\Program Files (x86)\Active Technologies\EXPERT RIDER AWG 4000\SCPI\AWG4KImportWaveforms\Sine0.txt",TXT
MMEMory:IMPort "Sine1","C:\Program Files (x86)\Active Technologies\EXPERT RIDER AWG 4000\SCPI\AWG4KImportWaveforms\Sine1.txt",TXT
MMEMory:IMPort "Sine2","C:\Program Files (x86)\Active Technologies\EXPERT RIDER AWG 4000\SCPI\AWG4KImportWaveforms\Sine2.txt",TXT
:SEQ:CHAN1:LENG 3;
:SEQ:CHAN2:LENG 3;
SOURce1:OUTputType DCAmplified
SOURce2:OUTputType DCAmplified
:SEQ:CHAN1:ELEM1:WAV "Sine0";:SEQ:CHAN1:ELEM1:REP INF;:SEQ:CHAN1:ELEM1:GOTO 1;:SEQ:CHAN1:ELEM1:WAITE NONE;:SEQ:CHAN1:ELEM1:JUMPE 0;:SEQ:CHAN1:ELEM1:JUMPType ASYNC;:SEQ:CHAN1:ELEM1:JUMPA 2;
:SEQ:CHAN1:ELEM2:WAV "Sine1";:SEQ:CHAN1:ELEM2:REP INF;:SEQ:CHAN1:ELEM2:GOTO 1;:SEQ:CHAN1:ELEM2:WAITE NONE;:SEQ:CHAN1:ELEM2:JUMPE 0;:SEQ:CHAN1:ELEM2:JUMPType ASYNC;:SEQ:CHAN1:ELEM2:JUMPA 3;
:SEQ:CHAN1:ELEM3:WAV "Sine2";:SEQ:CHAN1:ELEM3:REP INF;:SEQ:CHAN1:ELEM3:GOTO 1;:SEQ:CHAN1:ELEM3:WAITE NONE;:SEQ:CHAN1:ELEM3:JUMPE 0;:SEQ:CHAN1:ELEM3:JUMPType ASYNC;:SEQ:CHAN1:ELEM3:JUMPA 1;
:SEQ:CHAN2:ELEM1:WAV "Sine0";:SEQ:CHAN2:ELEM1:REP INF;:SEQ:CHAN2:ELEM1:GOTO 1;:SEQ:CHAN2:ELEM1:WAITE NONE;:SEQ:CHAN2:ELEM1:JUMPE 0;:SEQ:CHAN2:ELEM1:JUMPType ASYNC;:SEQ:CHAN2:ELEM1:JUMPA 2;
:SEQ:CHAN2:ELEM2:WAV "Sine1";:SEQ:CHAN2:ELEM2:REP INF;:SEQ:CHAN2:ELEM2:GOTO 1;:SEQ:CHAN2:ELEM2:WAITE NONE;:SEQ:CHAN2:ELEM2:JUMPE 0;:SEQ:CHAN2:ELEM2:JUMPType ASYNC;:SEQ:CHAN2:ELEM2:JUMPA 3;
:SEQ:CHAN2:ELEM3:WAV "Sine2";:SEQ:CHAN2:ELEM3:REP INF;:SEQ:CHAN2:ELEM3:GOTO 1;:SEQ:CHAN2:ELEM3:WAITE NONE;:SEQ:CHAN2:ELEM3:JUMPE 0;:SEQ:CHAN2:ELEM3:JUMPType ASYNC;:SEQ:CHAN2:ELEM3:JUMPA 1;
AWGControl:RUN