Talker Listener Script: <<Script1>>
*RST
AWGControl:CONFigure:CNUMber?
AWGControl:CONFigure:SEQuencer:MODE SIN;
AWGControl:CHANnel:FUNCTionality ARB,LOWSPeed;
AWGControl:RMODe SEQ;
WLIST:WAVeform:DELETE ALL
MMEMory:IMPort "wave1","C:\Program Files (x86)\Active Technologies\EXPERT RIDER AWG 4000\SCPI\AWG4KImportWaveforms\Sine2048.txt",TXT
MMEMory:IMPort "wave2","C:\Program Files (x86)\Active Technologies\EXPERT RIDER AWG 4000\SCPI\AWG4KImportWaveforms\Triangle2048.txt",TXT
EVENTS:TRIGINTIMERPeriod 1E6
ANALOGCHANnel1:EVENTS0:SOUrce1 TIMER;
ANALOGCHANnel1:EVENTS0:SOUrce2 TRUE;
ANALOGCHANnel1:EVENTS0:SOUrce3 TRUE;
ANALOGCHANnel1:EVENTS0:OPER1 AND;
ANALOGCHANnel1:EVENTS0:OPER2 AND;
ANALOGCHANnel1:EVENTS0:OPER3 AND;
SEQuence:CHANnel1:LENGth 2;:SEQuence:CHANnel2:LENGth 2
:SEQ:CHAN1:ELEM1:WAV "wave1";:SEQ:CHAN1:ELEM1:REP 10;:SEQ:CHAN1:ELEM1:GOTO 2;:SEQ:CHAN1:ELEM1:WAITE NONE;:SEQ:CHAN1:ELEM1:JUMPE NONE;:SEQ:CHAN1:ELEM1:JUMPType ASYNC;
:SEQ:CHAN1:ELEM2:WAV "wave2";:SEQ:CHAN1:ELEM2:REP 10;:SEQ:CHAN1:ELEM2:GOTO 1;:SEQ:CHAN1:ELEM2:WAITE 0;:SEQ:CHAN1:ELEM2:JUMPE NONE;:SEQ:CHAN1:ELEM2:JUMPType ASYNC;
:SEQ:CHAN2:ELEM1:WAV "wave1";:SEQ:CHAN2:ELEM1:REP 10;:SEQ:CHAN2:ELEM1:GOTO 2;:SEQ:CHAN2:ELEM1:WAITE NONE;:SEQ:CHAN2:ELEM1:JUMPE NONE;:SEQ:CHAN2:ELEM1:JUMPType ASYNC;
:SEQ:CHAN2:ELEM2:WAV "wave2";:SEQ:CHAN2:ELEM2:REP 10;:SEQ:CHAN2:ELEM2:GOTO 1;:SEQ:CHAN2:ELEM2:WAITE 0;:SEQ:CHAN2:ELEM2:JUMPE NONE;:SEQ:CHAN2:ELEM2:JUMPType ASYNC;
AWGControl:RUN
