Talker Listener Script: <<Script0>>
*RST
AWGControl:CONFigure:CNUMber?
AWGControl:CONFigure:SEQuencer:MODE SIN;
AWGControl:CHANnel:FUNCTionality ARB,LOWSPeed;
AWGControl:RMODe SEQ;
WLIST:WAVeform:DELETE ALL
MMEMory:IMPort "triangle","C:\Program Files (x86)\Active Technologies\EXPERT RIDER AWG 4000\SCPI\AWG4KImportWaveforms\Triangle.txt",TXT
MMEMory:IMPort "sinc","C:\Program Files (x86)\Active Technologies\EXPERT RIDER AWG 4000\SCPI\AWG4KImportWaveforms\Sinc.txt",TXT
MMEMory:IMPort "Sine0","C:\Program Files (x86)\Active Technologies\EXPERT RIDER AWG 4000\SCPI\AWG4KImportWaveforms\Sine0.txt",TXT
MMEMory:IMPort "Sine1","C:\Program Files (x86)\Active Technologies\EXPERT RIDER AWG 4000\SCPI\AWG4KImportWaveforms\Sine1.txt",TXT
MMEMory:IMPort "Sine2","C:\Program Files (x86)\Active Technologies\EXPERT RIDER AWG 4000\SCPI\AWG4KImportWaveforms\Sine2.txt",TXT
SLISt:SUBSequence:NEW "sub1",3;
SLISt:SUBSequence:CHANnel1:ELEMent1:WAVeform "sub1","Sine0"
SLISt:SUBSequence:CHANnel1:ELEMent2:WAVeform "sub1","triangle"
SLISt:SUBSequence:CHANnel1:ELEMent3:WAVeform "sub1","sinc"
SLISt:SUBSequence:CHANnel2:ELEMent1:WAVeform "sub1","Sine0"
SLISt:SUBSequence:CHANnel2:ELEMent2:WAVeform "sub1","triangle"
SLISt:SUBSequence:CHANnel2:ELEMent3:WAVeform "sub1","sinc"
SEQuence:LENgth 3;
SEQuence:CHANnel1:ELEMent1:WAVEform "Sine1" ;:SEQuence:CHANnel2:ELEMent1:WAVEform "Sine1"
SEQuence:ELEM1:REP 4;
SEQuence:ELEM2:SUBSequence "sub1";
SEQuence:ELEM2:REP 1;
SEQuence:CHANnel1:ELEMent3:WAVEform "Sine2";:SEQuence:CHANnel2:ELEMent3:WAVEform "Sine2"
SEQuence:ELEM3:REP 8;
SOURce1:OUTputType DCAmplified
SOURce2:OUTputType DCAmplified
AWGControl:RUN